# /etc/ppp/peers/gprs -- a example for use with a GPRS modem
#
# Change <user name> to the the one supplied by your provider and look
# at /etc/ppp/chat/gprs for some GPRS specific settings.  You'll also
# need to add your password to the /etc/ppp/chap-secrets or
# /etc/ppp/pap-secrets files.  If the connection doesn't work try
# changing some of the settings below.
#
# You'll also need to modify /etc/ppp/chat/gprs to include any AT
# commands for setting up the GPRS connection and to set the phone
# number to dial.
#
# You can then start/stop a connection with:
#   pon gprs
#   poff gprs
#
# Refer to the pppd(8) man page for more details.

/dev/ttyGPRS
115200

connect '/usr/sbin/chat -v -f /etc/ppp/chat/gprs'
disconnect '/usr/sbin/chat -v -f /etc/ppp/chat/disconnect'

user "foobar"
noauth

noipdefault
defaultroute
usepeerdns
noproxyarp

# PPP compression:
# PPP compression may be used between the phone and the pppd, but the
# serial connection is usually not the bottleneck in GPRS, so the
# compression is useless (and with some phones needs to disabled before
# the LCP negotiations succeed).
noaccomp
nobsdcomp
nodeflate
nopcomp
noaccomp

crtscts
modem

# No magic:
# Some phones may require this option.
#nomagic

# Require PAP authentication:
# Some phones may require this option.
#require-pap

# LCP echo requests:
# Some phones don't support LCP echo requests (PPP keep-alives)
# resulting pppd terminating the connection.
lcp-echo-interval 0

