# Example PPPD configuration for FONA GPRS connection on Debian/Ubuntu.

# MUST CHANGE: Change the -T parameter value **** to your network's APN value.
# For example if your APN is 'internet' (without quotes), the line would look like:
connect "/usr/sbin/chat -v -f /etc/chatscripts/gprs"

# MUST CHANGE: Uncomment the appropriate serial device for your platform below.
# For Raspberry Pi use /dev/ttyAMA0 by uncommenting the line below:
/dev/serial0

# Speed of the serial line.
115200

# Assumes that your IP address is allocated dynamically by the ISP.
noipdefault

# Try to get the name server addresses from the ISP.
usepeerdns

# Use this connection as the default route to the internet.
defaultroute

# Makes PPPD "dial again" when the connection is lost.
persist

# Do not ask the remote to authenticate.
noauth

# No hardware flow control on the serial link with FONA
nocrtscts

# No modem control lines with FONA.
local
